[DLG_102]
1000=系统初始化
1001=系统关闭
1002=打开图档文件
1003=关闭图档文件
1004=IO读取
1005=开始打标
1006=停止打标
1007=获取
1008=更改
1011=请输入别名：
1012=内容：
1014=移动
1015=旋转
1016=X偏移 / X旋转中心：
1017=Y偏移 / Y旋转中心：
1018=旋转角度：
1022=欢迎使用C++版二次开发Demo
1024=IO写入
1025=建议：与HLM/HGM一致。
1026=检测脚踏
1037=实时检测脚踏信号
1041=检测到的脚踏信号数：
1042=系统
1043=可变文本对象
1044=IO控制
1045=变换
1046=注意：“别名”是可变文本对象的“别名”，而不是“对象名”。
1047=重置视图
1048=视图控制：鼠标滚轮以缩放，按下滚轮并移动鼠标以拖动。
1035=获取狗ID信息
1036=集成商ID
1051=设备ID
1050=加密锁ID信息
1027=输出口IO读取
1055= 注:以上IO读取显示为十六进制
[STRINGTABLE]
System initialization succeeded!=初始化成功！
Another software is running=另一个程序在运行
The path is wrong=路径不正确,可能程序不在软件安装目录下运行
Initialize device failed!=初始化失败，请检查狗和卡的连接情况
Device was not initialized=未初始化
Command timeout=命令超时
The file can't be readed=无法读取文件
Specified font does not exist!=指定的字体不存在
Specified Layer does not exist!=指定的层号不存在
Specified Object not found!=没找到指定的对象
Parameter error..=参数非法
Operation are prohibted, Invalid state!=错误的状态,当前状态下不能执行此操作
Memory allocation failure!=分配内存失败
Out of mark range=打标范围超限
Insufficient buffer size=缓冲区不够
Null pointer..=空指针
No matched document!=未找到指定文档
Document has been opened!=指定文档已经被打开
Command execute failure!=下位机命令执行失败
Down multi document failed!=多文档数据下载失败
Document's Mandatory IO must not be same!=不能存相同的文档IO托管值
Document already downloaded in the card!=数据已下载
Call function error!=调用函数顺序不正确
Preprocess failed!=生成线条失败
No cali file,please start cali.exe first!=找不到校正文件，请先启动cali.exe进行校正
wheel data stop!=旋转切分停止
out of mark range!=超出打标范围
No Right!=没有二次开发库权限
Unknown error=未知错误
System initialization succeeded!=系统初始化成功！
System close succeeded!=系统关闭成功！
Open module file succeed!=打开图档文件成功！
Close module file succeed!=关闭图档文件成功！
Mark finish...!=打标完成！
Marking......!=正在打标......！
Mark finish...! It took =打标结束！耗时
Stop mark succeed!=停止打标成功！
Get object value succeed!=获取对象值成功！
Change object content succeed!=修改对象值成功！
Move succeed!=移动成功！
Rotate succeed!=旋转成功！
Read input port succeed!=读取IO成功！
Write output port succeed!=写入IO成功！
Touch trigger!=脚踏触发！
Touch is not triggered!=脚踏未触发！
Start check touch succeed!=启动实时检测脚踏信号成功！
Stop check touch succeed!=关闭实时检测脚踏信号成功！
Count of touch signal detected:=检测到的脚踏信号数：
Count of touch signal detected:0=检测到的脚踏信号数：0
A touch signal from the EMCC is received!=接收到一个来自EMCC卡的脚踏信息！
Language switch failed, please check the configuration file!=语言切换失败，请检查配置文件！